
--------------------------------------
Namco Classic Collection Vol. 1 (1995)
--------------------------------------
malcor



Location     Type          File ID      Checksum
~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~~
13D MAIN0   27C4096     NC1-MAIN0.ENG     B2DF   [ Program 0 ] [ English  ] 
14D MAIN1   27C4096     NC1-MAIN1.ENG     98A9   [ Program 1 ] [ English  ]
13D MAIN0   27C4096     NC1-MAIN0.JPN     9498   [ Program 0 ] [ Japanese ]
14D MAIN1   27C4096     NC1-MAIN1.JPN     0164   [ Program 1 ] [ Japanese ]
13D MAIN0   27C4096     NC1-MAIN0B.JPN    B15E   [ Program 0 ] [ Japanese ]
14D MAIN1   27C4096     NC1-MAIN1B.JPN    A88C   [ Program 1 ] [ Japanese ]

1C  SUB     27C4096     NC1-SUB           5B2C   [ Sub-Prog  ]
10C CG0     44pin 32meg Surface mounted        * [    GFX    ]
7B  VOICE   44pin 32meg Surface mounted        * [   Sound   ]
3C  KEYCUS  MACH210-15  Surface mounted        * [ KeyCustom ]


Note:  * - These ROMs were surface mounted and were not archived.
         - There are three different versions of the two main program
           ROMs. One English version and two Japanese versions.

         - Namco PCB:  ND-1 GAME PCB, hi-pric P41 B 
           8655960101, (8655970101)


Brief hardware overview:
------------------------

Main processor  - MC68HC000 12MHz    (68 pin QCC, surface mounted)
Sub-processor   - HD6413002F16 16MHz (100 pin PQFP microcontroller)
                - C416 custom
                - MACH210-15         (44 pin QCC switch matrix CPLD)
Sound processor - C352 Custom IC     (100 pin PQFP)
GFX             - YGV608-F           (100 pin PQFP, YAMAHA)
Video out       - LM1203N            (28 pin DIP, CRT output/drive preamp &
                                      comparitor) 


